\doxysection{src/\+Me\+Humiture\+Sensor.h File Reference}
\hypertarget{_me_humiture_sensor_8h}{}\label{_me_humiture_sensor_8h}\index{src/MeHumitureSensor.h@{src/MeHumitureSensor.h}}


Header for for \doxylink{_me_humiture_sensor_8cpp}{Me\+Humiture\+Sensor.\+cpp} module.  


{\ttfamily \#include $<$stdint.\+h$>$}\newline
{\ttfamily \#include $<$stdbool.\+h$>$}\newline
{\ttfamily \#include $<$Arduino.\+h$>$}\newline
{\ttfamily \#include "{}Me\+Config.\+h"{}}\newline
{\ttfamily \#include "{}Me\+Port.\+h"{}}\newline
Include dependency graph for Me\+Humiture\+Sensor.\+h\+:
\nopagebreak
\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=350pt]{_me_humiture_sensor_8h__incl}
\end{center}
\end{figure}
This graph shows which files directly or indirectly include this file\+:
\nopagebreak
\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=350pt]{_me_humiture_sensor_8h__dep__incl}
\end{center}
\end{figure}
\doxysubsubsection*{Classes}
\begin{DoxyCompactItemize}
\item 
class \mbox{\hyperlink{class_me_humiture}{Me\+Humiture}}
\begin{DoxyCompactList}\small\item\em Driver for humiture sensor device. \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
Header for for \doxylink{_me_humiture_sensor_8cpp}{Me\+Humiture\+Sensor.\+cpp} module. 

\begin{DoxyAuthor}{Author}
Make\+Block 
\end{DoxyAuthor}
\begin{DoxyVersion}{Version}
V1.\+0.\+1 
\end{DoxyVersion}
\begin{DoxyDate}{Date}
2015/11/18 
\end{DoxyDate}
\begin{DoxyParagraph}{Copyright}
This software is Copyright (C), 2012-\/2016, Make\+Block. Use is subject to license ~\newline
conditions. The main licensing options available are GPL V3 or Commercial\+: ~\newline
 
\end{DoxyParagraph}
\begin{DoxyParagraph}{Open Source Licensing GPL V3}
This is the appropriate option if you want to share the source code of your ~\newline
application with everyone you distribute it to, and you also want to give them ~\newline
the right to share who uses it. If you wish to use this software under Open ~\newline
Source Licensing, you must contribute all your source code to the open source ~\newline
community in accordance with the GPL Version 3 when your application is ~\newline
distributed. See \href{http://www.gnu.org/copyleft/gpl.html}{\texttt{ http\+://www.\+gnu.\+org/copyleft/gpl.\+html}}
\end{DoxyParagraph}
\begin{DoxyParagraph}{Description}
This file is a drive for humiture sensor device, It supports humiture sensor provided by the Make\+Block.
\end{DoxyParagraph}
\begin{DoxyParagraph}{Method List\+:}

\end{DoxyParagraph}

\begin{DoxyEnumerate}
\item void \doxylink{class_me_humiture_a3d96abbe15a836cfae534ec67f908f85}{Me\+Humiture\+::setpin(uint8\+\_\+t port)}
\item void \doxylink{class_me_humiture_aa407c9adbdefaab8cf419d9748a11e56}{Me\+Humiture\+::update(void)}
\item uint8\+\_\+t \doxylink{class_me_humiture_a8e2e8567ea52c7bea8148214636e5444}{Me\+Humiture\+::get\+Humidity(void)}
\item uint8\+\_\+t \doxylink{class_me_humiture_a5811d17c07807b9617751adf382abf15}{Me\+Humiture\+::get\+Temperature(void)}
\item uint8\+\_\+t \doxylink{class_me_humiture_a0aa1f08444d67c6bed1c3eb0f357afa7}{Me\+Humiture\+::get\+Value(uint8\+\_\+t index)}
\item double \doxylink{class_me_humiture_a2b70560a4598ec78832b13dfc63fdd07}{Me\+Humiture\+::get\+Fahrenheit(void)}
\item double \doxylink{class_me_humiture_ae42e2c3fac7b1e53c0732d278de880c1}{Me\+Humiture\+::get\+Kelvin(void)}
\item double \doxylink{class_me_humiture_af89ec5b9a23973e9256c8458c340f067}{Me\+Humiture\+::getdew\+Point(void)}
\item double \doxylink{class_me_humiture_aad97cff43721852a7e2d72cd223d1d3f}{Me\+Humiture\+::get\+Point\+Fast()}
\end{DoxyEnumerate}

\begin{DoxyParagraph}{History\+:}

\begin{DoxyPre}
`<Author>`         `<Time>`        `<Version>`        `<Descr>`
Mark Yan         2015/09/08          1.0.0            Rebuild the old lib.
forfish          2015/11/18          1.0.1            Add some functions.
lanweiting       2017/07/11          1.0.2            function update() add delay more time
\end{DoxyPre}
 
\end{DoxyParagraph}
