Data Structures | Typedefs | Functions
acc_detector_presence.h File Reference
`#include <stdbool.h>`
`#include <stddef.h>`
`#include <stdint.h>`
`#include "acc_definitions_a121.h"`
`#include "acc_definitions_common.h"`
`#include "acc_processing.h"`
`#include "acc_sensor.h"`

Go to the source code of this file.

## Data Structures
struct | acc_detector_presence_result_t
| Presence detector results container. More...
struct | acc_detector_presence_metadata_t

## Typedefs
typedef struct acc_detector_presence_handle | acc_detector_presence_handle_t
typedef struct acc_detector_presence_config | acc_detector_presence_config_t

## Functions
acc_detector_presence_config_t * | acc_detector_presence_config_create (void)
| Create a configuration for a presence detector. More...
void | acc_detector_presence_config_destroy (acc_detector_presence_config_t *presence_config)
| Destroy a presence detector configuration. More...
void | acc_detector_presence_config_log (const acc_detector_presence_config_t *presence_config)
| Print a configuration to the log. More...
bool | acc_detector_presence_get_buffer_size (const acc_detector_presence_handle_t *presence_handle, uint32_t *buffer_size)
| Get the buffer size needed for the provided presence detector handle. More...
acc_detector_presence_handle_t * | acc_detector_presence_create (acc_detector_presence_config_t *presence_config, acc_detector_presence_metadata_t *metadata)
| Create a presence detector with the provided configuration. More...
void | acc_detector_presence_destroy (acc_detector_presence_handle_t *presence_handle)
| Destroy a presence detector identified with the provided handle. More...
bool | acc_detector_presence_prepare (acc_detector_presence_handle_t *presence_handle, acc_detector_presence_config_t *presence_config, acc_sensor_t *sensor, const acc_cal_result_t *cal_result, void *buffer, uint32_t buffer_size)
| Prepare the detector to do a measurement. More...
bool | acc_detector_presence_process (acc_detector_presence_handle_t *presence_handle, void *buffer, acc_detector_presence_result_t *result)
| Process the data according to the configuration used in acc_detector_presence_config_create. More...
void | acc_detector_presence_config_start_set (acc_detector_presence_config_t *presence_config, float start)
| Set the start point of measurement interval in meters. More...
float | acc_detector_presence_config_start_get (const acc_detector_presence_config_t *presence_config)
| Get the start point of measurement interval in meters. More...
void | acc_detector_presence_config_end_set (acc_detector_presence_config_t *presence_config, float end)
| Set the end point of measurement interval in meters. More...
float | acc_detector_presence_config_end_get (const acc_detector_presence_config_t *presence_config)
| Get the end point of measurement interval in meters. More...
void | acc_detector_presence_config_step_length_set (acc_detector_presence_config_t *presence_config, uint16_t step_length)
| Set the step length in points. More...
uint16_t | acc_detector_presence_config_step_length_get (const acc_detector_presence_config_t *presence_config)
| Get the step length in points. More...
void | acc_detector_presence_config_auto_step_length_set (acc_detector_presence_config_t *presence_config, bool enable)
| Enable automatic selection of step length based on the profile. More...
bool | acc_detector_presence_config_auto_step_length_get (const acc_detector_presence_config_t *presence_config)
| Get if automatic selection of step length based on the profile is enabled. More...
void | acc_detector_presence_config_profile_set (acc_detector_presence_config_t *presence_config, acc_config_profile_t profile)
| Set a profile. More...
acc_config_profile_t | acc_detector_presence_config_profile_get (const acc_detector_presence_config_t *presence_config)
| Get the currently set profile. More...
void | acc_detector_presence_config_auto_profile_set (acc_detector_presence_config_t *presence_config, bool enable)
| Enable automatic selection of profile based on start point of measurement. More...
bool | acc_detector_presence_config_auto_profile_get (const acc_detector_presence_config_t *presence_config)
| Get if automatic selection of profile based on start point of measurement is enabled. More...
void | acc_detector_presence_config_inter_frame_idle_state_set (acc_detector_presence_config_t *presence_config, acc_config_idle_state_t idle_state)
| Set inter frame idle state. More...
acc_config_idle_state_t | acc_detector_presence_config_inter_frame_idle_state_get (const acc_detector_presence_config_t *presence_config)
| Get inter frame idle state. More...
void | acc_detector_presence_config_hwaas_set (acc_detector_presence_config_t *presence_config, uint16_t hwaas)
| Set the hardware accelerated average samples (HWAAS) More...
uint16_t | acc_detector_presence_config_hwaas_get (const acc_detector_presence_config_t *presence_config)
| Get the hardware accelerated average samples (HWAAS) More...
void | acc_detector_presence_config_sweeps_per_frame_set (acc_detector_presence_config_t *presence_config, uint16_t sweeps_per_frame)
| Set the number of sweeps per frame. More...
uint16_t | acc_detector_presence_config_sweeps_per_frame_get (const acc_detector_presence_config_t *presence_config)
| Get the number of sweeps per frame. More...
void | acc_detector_presence_config_frame_rate_set (acc_detector_presence_config_t *presence_config, float frame_rate)
| Set the frame rate. More...
float | acc_detector_presence_config_frame_rate_get (const acc_detector_presence_config_t *presence_config)
| Get the frame rate. More...
void | acc_detector_presence_config_frame_rate_app_driven_set (acc_detector_presence_config_t *presence_config, bool enable)
| Set if the application should maintain the requested frame rate. More...
bool | acc_detector_presence_config_frame_rate_app_driven_get (const acc_detector_presence_config_t *presence_config)
| Get if the application should maintain the requested frame rate. More...
void | acc_detector_presence_config_sensor_set (acc_detector_presence_config_t *presence_config, acc_sensor_id_t sensor_id)
| Set sensor ID. More...
acc_sensor_id_t | acc_detector_presence_config_sensor_get (const acc_detector_presence_config_t *presence_config)
| Get sensor ID. More...
void | acc_detector_presence_config_reset_filters_on_prepare_set (acc_detector_presence_config_t *presence_config, bool enable)
| Set if the presence filters should reset on prepare. More...
bool | acc_detector_presence_config_reset_filters_on_prepare_get (const acc_detector_presence_config_t *presence_config)
| Get if the presence filters should reset on prepare. More...
void | acc_detector_presence_config_inter_frame_presence_timeout_set (acc_detector_presence_config_t *presence_config, uint16_t inter_frame_presence_timeout)
| Set the inter-frame presence timeout in seconds. More...
uint16_t | acc_detector_presence_config_inter_frame_presence_timeout_get (const acc_detector_presence_config_t *presence_config)
| Get the inter-frame presence timeout in seconds. More...
void | acc_detector_presence_config_inter_phase_boost_set (acc_detector_presence_config_t *presence_config, bool enable)
| Set inter-frame phase boost. More...
bool | acc_detector_presence_config_inter_phase_boost_get (const acc_detector_presence_config_t *presence_config)
| Get if inter-frame phase boost is enabled. More...
void | acc_detector_presence_config_intra_detection_set (acc_detector_presence_config_t *presence_config, bool enable)
| Set intra-frame presence detection. More...
bool | acc_detector_presence_config_intra_detection_get (const acc_detector_presence_config_t *presence_config)
| Get if frame intra-frame presence detection is enabled. More...
void | acc_detector_presence_config_intra_detection_threshold_set (acc_detector_presence_config_t *presence_config, float intra_detection_threshold)
| Set the detection threshold for the intra-frame presence detection. More...
float | acc_detector_presence_config_intra_detection_threshold_get (const acc_detector_presence_config_t *presence_config)
| Get the detection threshold for the intra-frame presence detection. More...
void | acc_detector_presence_config_inter_detection_set (acc_detector_presence_config_t *presence_config, bool enable)
| Set inter-frame presence detection. More...
bool | acc_detector_presence_config_inter_detection_get (const acc_detector_presence_config_t *presence_config)
| Get if inter-frame presence detection is enabled. More...
void | acc_detector_presence_config_inter_detection_threshold_set (acc_detector_presence_config_t *presence_config, float inter_detection_threshold)
| Set the detection threshold for the inter-frame presence detection. More...
float | acc_detector_presence_config_inter_detection_threshold_get (const acc_detector_presence_config_t *presence_config)
| Get the detection threshold for the inter-frame presence detection. More...
void | acc_detector_presence_config_inter_frame_deviation_time_const_set (acc_detector_presence_config_t *presence_config, float inter_frame_deviation_time_const)
| Set the time constant of the low pass filter for the inter-frame deviation between fast and slow. More...
float | acc_detector_presence_config_inter_frame_deviation_time_const_get (const acc_detector_presence_config_t *presence_config)
| Get the time constant of the low pass filter for the inter-frame deviation between fast and slow. More...
void | acc_detector_presence_config_inter_frame_fast_cutoff_set (acc_detector_presence_config_t *presence_config, float inter_frame_fast_cutoff)
| Set the cutoff frequency of the low pass filter for the fast filtered absolute sweep mean. More...
float | acc_detector_presence_config_inter_frame_fast_cutoff_get (const acc_detector_presence_config_t *presence_config)
| Get the cutoff frequency of the low pass filter for the fast filtered absolute sweep mean. More...
void | acc_detector_presence_config_inter_frame_slow_cutoff_set (acc_detector_presence_config_t *presence_config, float inter_frame_slow_cutoff)
| Set the cutoff frequency of the low pass filter for the slow filtered absolute sweep mean. More...
float | acc_detector_presence_config_inter_frame_slow_cutoff_get (const acc_detector_presence_config_t *presence_config)
| Get the cutoff frequency of the low pass filter for the slow filtered absolute sweep mean. More...
void | acc_detector_presence_config_intra_frame_time_const_set (acc_detector_presence_config_t *presence_config, float intra_frame_time_const)
| Set the time constant for the depthwise filtering in the intra-frame part. More...
float | acc_detector_presence_config_intra_frame_time_const_get (const acc_detector_presence_config_t *presence_config)
| Get the time constant for the depthwise filtering in the intra-frame part. More...
void | acc_detector_presence_config_intra_output_time_const_set (acc_detector_presence_config_t *presence_config, float intra_output_time_const)
| Set the time constant for the output in the intra-frame part. More...
float | acc_detector_presence_config_intra_output_time_const_get (const acc_detector_presence_config_t *presence_config)
| Get the time constant for the output in the intra-frame part. More...
void | acc_detector_presence_config_inter_output_time_const_set (acc_detector_presence_config_t *presence_config, float inter_output_time_const)
| Set the time constant for the output in the inter-frame part. More...
float | acc_detector_presence_config_inter_output_time_const_get (const acc_detector_presence_config_t *presence_config)
| Get the time constant for the output in the inter-frame part. More...