Macros | Functions
example_detector_distance_low_power_hibernate.c File Reference
`#include <stdbool.h>`
`#include <stdint.h>`
`#include <stdio.h>`
`#include <stdlib.h>`
`#include "acc_definitions_a121.h"`
`#include "acc_definitions_common.h"`
`#include "acc_detector_distance.h"`
`#include "acc_hal_definitions_a121.h"`
`#include "acc_hal_integration_a121.h"`
`#include "acc_integration.h"`
`#include "acc_integration_log.h"`
`#include "acc_rss_a121.h"`
`#include "acc_sensor.h"`
`#include "acc_version.h"`

Go to the source code of this file.

## Macros
#define | SENSOR_ID (1U)
#define | SENSOR_TIMEOUT_MS (1000U)
#define | DEFAULT_UPDATE_RATE (1.0f)

## Functions
static void | print_result (acc_detector_distance_result_t *result)
static void | cleanup (acc_detector_distance_handle_t *distance_handle, acc_detector_distance_config_t *distance_config, acc_sensor_t *sensor, void *buffer, void *calibration_buffer)
static void | set_config (acc_detector_distance_config_t *distance_config)
int | acconeer_main (int argc, char *argv[])
| Assembly test example. More...

## Macro Definition Documentation

## ◆ DEFAULT_UPDATE_RATE

#define DEFAULT_UPDATE_RATE (1.0f)

Examples
  example_detector_distance_low_power_hibernate.c.

Definition at line 51 of file example_detector_distance_low_power_hibernate.c.

## ◆ SENSOR_ID

#define SENSOR_ID (1U)

Examples
  example_detector_distance_low_power_hibernate.c.

Definition at line 49 of file example_detector_distance_low_power_hibernate.c.

## ◆ SENSOR_TIMEOUT_MS

#define SENSOR_TIMEOUT_MS (1000U)

Examples
  example_detector_distance_low_power_hibernate.c.

Definition at line 50 of file example_detector_distance_low_power_hibernate.c.

## Function Documentation

## ◆ acconeer_main()

int acconeer_main | ( | int | argc,
|  | char * | argv[]
| ) |  |

Assembly test example.

Surface velocity example application.

Tank level reference application.

Smart presence reference application.

Breathing example application.

Service subsweeps example.

Service multple configurations example.

Low power service example.

Service example.

Processing subtract adaptive background example.

Processing static presence example.

Processing peak interpolation example.

Processing noncoherent mean example.

Processing coherent mean example.

Processing amplitude example.

Detector presence example with multiple configurations.

Low power detector presence example.

Detector presence example.

Distance detector low power example.

Detector distance example.

Control helper example.

Returns
  Returns EXIT_SUCCESS if successful, otherwise EXIT_FAILURE

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Test if measure on wake up is enable Do a measurement if the the detector is ready (configured and calibrated)

Examples
  example_detector_distance_low_power_hibernate.c.

Definition at line 70 of file example_detector_distance_low_power_hibernate.c.

## ◆ cleanup()

static void cleanup | ( | acc_detector_distance_handle_t * | distance_handle,
|  | acc_detector_distance_config_t * | distance_config,
|  | acc_sensor_t * | sensor,
|  | void * | buffer,
|  | void * | calibration_buffer
| ) |  |
| static

Examples
  example_detector_distance_low_power_hibernate.c.

Definition at line 294 of file example_detector_distance_low_power_hibernate.c.

## ◆ print_result()

static void print_result | ( | acc_detector_distance_result_t * | result | ) |
| static

Examples
  example_detector_distance_low_power_hibernate.c.

Definition at line 339 of file example_detector_distance_low_power_hibernate.c.

## ◆ set_config()

static void set_config | ( | acc_detector_distance_config_t * | distance_config | ) |
| static

Examples
  example_detector_distance_low_power_hibernate.c.

Definition at line 330 of file example_detector_distance_low_power_hibernate.c.