# SensorBlue/Oria/Brifit ThermoBeacon

|Model Id|[WS02/WS08](https://github.com/theengs/decoder/blob/development/src/devices/ThermoBeacon_json.h)|
|-|-|
|Brand|SensorBlue/Oria/Brifit|
|Model|ThermoBeacon|
|Short Description|Temperature and humidity sensor, various models sold under various brands|
|Communication|BLE broadcast|
|Frequency|2.4Ghz|
|Power Source|CR2032/CR2477|
|Exchanged Data|temperature, humidity, voltage, timestamp, maximum temperature, maximum temperature timestamp, minimum temperature, minimum temperature timestamp|
|Encrypted|No|

All timestamps are the number of seconds since the device is powered on. The minimum and maximum temperatures are also the values since the device is powered on.
