MAX30001G 1.0.1 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
max30001_cnfg_rtor1_reg_t Union Reference

CNFG_RTOR1 (0x1D) page 59. More...

`#include <max30001g_regs_typedefs.h>`

## Public Attributes
uint32_t | all
struct {
uint32_t en_rtor: 1
uint32_t gain: 4
uint32_t pavg: 2
uint32_t ptsf: 4
uint32_t reserved: 8
uint32_t reserved1: 8
uint32_t reserved2: 1
uint32_t wndw: 4
} | bit

## Detailed Description

CNFG_RTOR1 (0x1D) page 59.

## Member Data Documentation

## ◆ all

uint32_t max30001_cnfg_rtor1_reg_t::all

## ◆

struct { ... } max30001_cnfg_rtor1_reg_t::bit

## ◆ en_rtor

uint32_t max30001_cnfg_rtor1_reg_t::en_rtor

## ◆ gain

uint32_t max30001_cnfg_rtor1_reg_t::gain

## ◆ pavg

uint32_t max30001_cnfg_rtor1_reg_t::pavg

## ◆ ptsf

uint32_t max30001_cnfg_rtor1_reg_t::ptsf

## ◆ reserved

uint32_t max30001_cnfg_rtor1_reg_t::reserved

## ◆ reserved1

uint32_t max30001_cnfg_rtor1_reg_t::reserved1

## ◆ reserved2

uint32_t max30001_cnfg_rtor1_reg_t::reserved2

## ◆ wndw

uint32_t max30001_cnfg_rtor1_reg_t::wndw

The documentation for this union was generated from the following file:

- src/max30001g_regs_typedefs.h