MAX30001G 1.0.1 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
max30001_cnfg_rtor2_reg_t Union Reference

CNFG_RTOR2 (0x1E) page 59. More...

`#include <max30001g_regs_typedefs.h>`

## Public Attributes
uint32_t | all
struct {
uint32_t hoff: 6
uint32_t ravg: 2
uint32_t reserved: 8
uint32_t reserved1: 8
uint32_t reserved2: 1
uint32_t reserved3: 2
uint32_t reserved4: 2
uint32_t rhsf: 3
} | bit

## Detailed Description

CNFG_RTOR2 (0x1E) page 59.

## Member Data Documentation

## ◆ all

uint32_t max30001_cnfg_rtor2_reg_t::all

## ◆

struct { ... } max30001_cnfg_rtor2_reg_t::bit

## ◆ hoff

uint32_t max30001_cnfg_rtor2_reg_t::hoff

## ◆ ravg

uint32_t max30001_cnfg_rtor2_reg_t::ravg

## ◆ reserved

uint32_t max30001_cnfg_rtor2_reg_t::reserved

## ◆ reserved1

uint32_t max30001_cnfg_rtor2_reg_t::reserved1

## ◆ reserved2

uint32_t max30001_cnfg_rtor2_reg_t::reserved2

## ◆ reserved3

uint32_t max30001_cnfg_rtor2_reg_t::reserved3

## ◆ reserved4

uint32_t max30001_cnfg_rtor2_reg_t::reserved4

## ◆ rhsf

uint32_t max30001_cnfg_rtor2_reg_t::rhsf

The documentation for this union was generated from the following file:

- src/max30001g_regs_typedefs.h