MAX30001G 1.3.0 Arduino library for MAX30001G ECG and BIOZ AFE

Public Attributes | List of all members
max30001_cnfg_bioz_lc_reg_t Union Reference

CNFG_BIOZ_LC (0x1A) page 57. More...

`#include <max30001g_regs_typedefs.h>`

## Public Attributes
uint32_t | all
struct {
uint32_t bistr: 2
uint32_t cmag_lc: 4
uint32_t cmres: 4
uint32_t en_bistr: 1
uint32_t hi_lob: 1
uint32_t lc2x: 1
uint32_t reserved1: 4
uint32_t reserved2: 4
uint32_t reserved3: 3
uint32_t reserved4: 8
} | bit

## Detailed Description

CNFG_BIOZ_LC (0x1A) page 57.

## Member Data Documentation

## ◆ all

uint32_t max30001_cnfg_bioz_lc_reg_t::all

## ◆ bistr

uint32_t max30001_cnfg_bioz_lc_reg_t::bistr

## ◆

struct { ... } max30001_cnfg_bioz_lc_reg_t::bit

## ◆ cmag_lc

uint32_t max30001_cnfg_bioz_lc_reg_t::cmag_lc

## ◆ cmres

uint32_t max30001_cnfg_bioz_lc_reg_t::cmres

## ◆ en_bistr

uint32_t max30001_cnfg_bioz_lc_reg_t::en_bistr

## ◆ hi_lob

uint32_t max30001_cnfg_bioz_lc_reg_t::hi_lob

## ◆ lc2x

uint32_t max30001_cnfg_bioz_lc_reg_t::lc2x

## ◆ reserved1

uint32_t max30001_cnfg_bioz_lc_reg_t::reserved1

## ◆ reserved2

uint32_t max30001_cnfg_bioz_lc_reg_t::reserved2

## ◆ reserved3

uint32_t max30001_cnfg_bioz_lc_reg_t::reserved3

## ◆ reserved4

uint32_t max30001_cnfg_bioz_lc_reg_t::reserved4

The documentation for this union was generated from the following file:

- src/max30001g_regs_typedefs.h